Government of the People’s Republic of Bangladesh

National Board of Revenue

Segunbagicha, Dhaka

www.nbr.gov.bd

File No: 08.01.000.066.07.007.20/314 Date: 17.12.2020

This is notifying to all concern that the following Amendments are made to the Tender Ref No. 08.01.0000.066.07.007.20, Package: 04: ***Supply, Installation and commissioning of Database Software, SOClass License, Backup Solution and other necessary servers and laptop.***, published on: 26/11/2020.

***Amendments on Tender Last Selling Date, Closing Date and Time and Opening Date and Time:***

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Tender Information** | | ***Existing As*** | | | ***Changed As*** | | |
| # | Package No | Package Name | Last Selling Date | Closing Date and Time | Opening Date and Time | **Last Selling Date** | **Closing Date and Time** | **Opening Date and Time** |
| 1 | Package- 04 | Supply, Installation and commissioning of Database Software, SOClass License, Backup Solution and other necessary servers and laptop | 20.12.2020 | 20.12.2020  02:00 PM | 20.12.2020 02:30 PM | **28.12.2020** | **28.12.2020**  **02:00 PM** | **28.12.2020**  **02:30 PM** |

***Amendments on Tender Specifications***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Section** | **Page** | **Existing Information** | **Amendment** |
| 1 | 7  A4: Systems Specifications  1: Servers | 78 | Network Interface Onboard  Minimum Four onboard auto-sensing 100/1000/10000 Base-T Ethernet ports | **Network Interface Onboard**  **Two1/10GbE ports (RJ45) & two 1/10/25 GbE ports (SFP28) onboard** |
| 2 | 7  A4: Systems Specifications  1: Servers | 77 | RAID Controller  12 Gb/sec SAS-3 RAID HBA supporting levels: 0, 1, 5, 6, 10, 50, and 60 | **RAID Controller**  **12 Gb/sec SAS-3 RAID HBA supporting levels: 0, 1, 5, 6, 10, 50, and 60 with 2GB of flash-backed write-back cache** |
| 3 | 7  A4: Systems Specifications  1: Servers | 77 |  | **Server Rack Unit: 1U** |
| 4 | 7  A4: Systems Specifications | 78 | Hard Disk Drive  2.4 TB 10000 rpm 2.5-inch SAS-3 HDD Hot-Pluggable Hard Disk Drives | **Hard Disk Drive**  **1.2 TB 10000 rpm 2.5-inch SAS-3 HDD Hot-Pluggable Hard Disk Drives**  **Minimum 4 x 1.2 TB SAS HDD** |
| 5 | 7  A6: Backup Solution Specifications | 110-111 | Front-End and Backend connectivity  The proposed unified storage system should have minimum 4 x 16Gb FC Ports for host connectivity per controller/node. Single controller/node of storage system should offer 96 Gbps of aggregate bandwidth for disk drive connectivity. | **Frontend and Backend Connectivity**  **The proposed Unified Storage system should have a minimum 2 X 16 Gbps FC ports for host connectivity and 2 X 10Gbps SFP+ ports per controller/node. Single Controller/Node of the storage system should offer 96 Gbps of aggregate bandwidth for disk drive connectivity** |
| 6 | 7 A5: Network Equipment for Emergency Stock Specifications | 86 | Expansion Slot  Min. 2 Network Interface Module Slots | **Omit** |
| 7 | Cover Page | 1 | Invitation for Tender No: 08.01.0000.091.53.001.19.149 | **Invitation for Tender No: 08.01.0000.066.07.007.20** |
| 8 | ITT 28.1(f) | 30 | Manufacturer’s Authorization is required only for the following items listed in Section 6: Schedule of Requirements:  A.1: List of Servers & Storage | **Manufacturer’s Authorization is required only for the following items listed in Section 6: Schedule of Requirements:**  **A.1: List of Database Software**  **2. Oracle Business Intelligence**  **A.4: List of Systems**   1. **Servers for AW Peripheral Services** 2. **SAN Switch**   **A.5: List of Network Equipment for Emergency Stock**   1. **WAN Router** 2. **Branch Firewall** 3. **Branch Switch**   **A.6: List of Backup Solution** |
| 9 | 7 A.1: Database Software Specifications | 70-72 |  | **Support Renewal Start Date 01 July 2021 and End Date 30 June 2024.** |

**(Syed Golam Kibria)**

Member (Customs: Policy & ICT)

National Board of Revenue Segunbagicha, Dhaka.